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SOP 22  |  Property setup
Start a mobile property setup walk
Start an authorized setup recording before marking the unit route.
For Mobile · Administrator / Supervisor
Before you start Use the approved sensor-capable app build, a registered device, setup permission and reviewed boundary. Clock out of routine tracking first.
Open Manage > Property > Property readiness & setup runs
Step 1 Choose the property
Open its setup task. Read property instructions or What is recorded? and confirm the address.
Step 2 Choose recording mode
Choose Screen-off or Screen-on only and read the consent text. Screen-on recording pauses when the app is left or the phone locks.
Step 3 Check your position
Tap Show my live position. Allow the requested precise location permissions and move safely to the authorized start area.
Step 4 Start the recording
When start checks pass, use Agree & start background setup or Start screen-on setup. The button depends on the selected mode.
Step 5 Choose phone position
Select where you will carry the phone and keep it there while walking. Confirm the app shows the active setup walk.
Check your result Walk to the next unit is available and recording status is shown for the selected property.
If something goes wrong A map preview is not a started setup run. If sensors, permission or boundary checks fail, resolve the displayed issue before starting.
See the picture reference on the next page.


SOP 22  Picture reference
Start a mobile property setup walk
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Step 2 · A live map preview does not start recording. Use the authorized start action.
Workflow illustration. Follow the complete numbered instructions on the previous page.
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Start a mobile property setup walk

Choose Screen-off or Check permission and  Start the authorized Choose consistent
Screen-on position recording phone position

Alive map preview does not start recording. Use the authorized start action.

DK VALET WORKFORCE - Follow the numbered procedure for the complete instructions.








